/********************************\
|				 |
|   http:\\www.BruceWiggins.co.uk|                           
|   Wigware Ambisonic Encoder 2o |
|      Version 0.91		 |
|	   27-11-2014		 |
|				 |
\********************************/

0. You use this software at your own risk, I cannot
   and willnot be held responsible for any adverse effects
   this software causes.....IT IS STILL IN THE BETA STAGE
   OF DEVELOPMENT (not that it should do, however ;-)
1. Unzip the plugin file into your VST plugin directory
   (normally library/audio/plugins/vst)
2. For PERSONAL AND EDUCATIONAL USE ONLY.
3. If you wish to use this software for research and/or
   commercial activities, contact me b.j.wiggins@derby.ac.uk
   (I’m interested as to how and where it’s used!)

These plug-ins take a mono input and output the five (2D) or 9 (3D) channels
of 2nd order B Format.  If NFC (near field compensation) is set
to OFF then as the source is moved into the middle, the directional
components are turned down (centre sources comes out of every speaker
equally when decoded).  If NFC is set to a distance, then the 
distance parameter then controls the distance filtering which
applies LF boost (proximity effect) as the source moves closer
to the middle.  This will be a subtle thing for 1st order, but
is included for research purposes!

Any questions, visit the website and ask away!